# Implementation of the Dynamic TOPMODEL Hydrological Model

## Documentation for package ‘dynatopmodel’ version 1.1

- DESCRIPTION file.
- Package NEWS.

## Help Pages

dynatopmodel-package | Implementation of the Dynamic TOPMODEL hydrological model.
aggregate_obs | Resample observation data at a new time interval
approx.pe.ts | Create sinsuiodal time series of potential evapotranspiration input
brompton | Topographic and observation data for running Dynamic TOPMODEL.
build_chans | Construct a raster of channel locations from vector or topographic data
build_layers | Construct basic landscape layer data for Dynamic TOPMODEL run
build_routing_table | Generate a network routing table
discretise | Discrete a catchment into hydrological response units (HRUs)
disp.par | Default list of parameters to control the graphical output during model simulation and via disp.output
disp_output | Display output of a Dynamic TOPMODEL run
dynatopmodel | Implementation of the Dynamic TOPMODEL hydrological model.
NSE | Nash Sutcliffe Efficiency of a model's output against observations
run.dtm | Run Dynamic TOPMODEL using the catchment areal groupings (response units) for a discretisation.
time_at_peak | Time of maximum observation
time_to_peak | Time between the peak rainfall and the peak discharge
upslope.area | Upslope contributing area and wetness index calculation