ReacTran-package        Reactive transport modelling in 1D, 2D and 3D
advection.1D            One-Dimensional Advection Equation
fiadeiro                Advective Finite Difference Weights
g.sphere                Surface Area and Volume of Geometrical Objects
p.exp                   Common Properties with Distance, to be used
                        with setup.prop.1D
setup.compaction.1D     Calculates Advective Velocities of the Pore
                        Water and Solid Phase in a Water Saturated
                        Sediment assuming Steady State Compaction
setup.grid.1D           Creates a One-Dimensional Finite Difference
                        Grid
setup.grid.2D           Creates a Finite Difference Grid over a
                        Two-Dimensional Rectangular Domain
setup.prop.1D           Attaches a Property to a One-Dimensional Grid
setup.prop.2D           Attaches a Property to a Two-Dimensional Grid
tran.1D                 General One-Dimensional Advective-Diffusive
                        Transport
tran.2D                 General Two-Dimensional Advective-Diffusive
                        Transport
tran.3D                 General Three-Dimensional Advective-Diffusive
                        Transport
tran.cylindrical        Diffusive Transport in cylindrical (r, theta,
                        z) and spherical (r, theta, phi) coordinates.
tran.polar              Diffusive Transport in polar (r, theta)
                        coordinates.
tran.volume.1D          1-D, 2-D and 3-D Volumetric Advective-Diffusive
                        Transport in an Aquatic System
